



**Pick Up**

**Focus**

**Raspberry Pi with NFC Controller (PN532)**

**Request Items**

Confirm order using unique identifier

**Server**

Send unique identifier over HTTP

On arrival to pick up, send over a unique identifier over NFC via I2C

Confirm an Order over HTTP

Request an Order over HTTP

